#

The drawing shows a feedline connected to a load, Z sub L. The input impedance is Z sub in while feedline impedance is Z sub 01. A lambda over 4 transformer is inserted in-series between feedline and load, connecting terminals M, M-prime and B, B-prime, with the distance between B, B-prime, and A, A-prime labeled d. The transformer impedance is labeled Z sub 02, while the impedance of the transmission line between B and A is Z of d.