#

The top of the screen shows a circuit diagram for a transmission line of length, d equals 0.193 lambda or 57.9 meters, that connects a generator and a load. The generator has a voltage source labeled V-tilde sub g equals 1.0 plus j 0.0 V, and impedance labeled Z sub g equals 100.0 plus j 0.0 ohms, while the load impedance is Z sub L equals 100.0 plus j 0.0 ohms. The impedance of the transmission line is Z sub 0 equals 50.0 plus j 0.0 ohms, while other parameters are labeled epsilon sub r equals 1.0, f equals 1.0 Gigahertz, and lambda equals 300.0 millimeters. The same parameter values are indicated in the fields shown in the lower panels.