#

The top left screen of the module shows a circuit in which a lossless transmission line connects a generator with a load, R sub L. The generator shows a voltage source, V sub g with a resistance R sub g. An input waveform shows square waves with amplitude labeled V sub g max.

The bottom left screen shows a graph plotting V sub T against T. The rectangular waveform is irregular, ranging between 200.0 V and negative 150.0 V in the beginning, and tapering down to 25 V at 4 T, and plus or minus 1 V at 8 T.

The right part of the module shows the following parameters for set load and data:

Set load:

R sub L equals 10.0 ohms (with resistance button selected)

Set Generator:

V sub g max equals 1.0 V; R sub g equals 100.0 ohms

Data:

Pulse input: gamma equals 160.0 p s

Cursor: z equals 48.93 m m

Transit time: Input to load: T equals 333.3333 p s

Transit time: Input to cursor position: T sub c equals 163.1 p s

Transit time: Input to load and back to cursor: T sub L C equals 503.56667 p s

Phase velocity: u sub p equals 3.0 times 10 raised to 9 m per s

Reflection coefficients: Gamma sub 0 equals 0.6; Gamma sub L equals 0.6667