#

The illustration shows a junction made by the copper and bismuth wires at one end that indicates measurement junction or T sub 2. The other ends of the copper and bismuth are connected with a resistor at the positive and negative terminal respectively. The junction between the conducting materials and resistor is labeled cold reference junction T sub 1. A Seebeck potential V sub s is generated across the resistor and a current I flows clockwise in the circuit.