#

The diagram shows two duplexers that are placed one above each other. The first duplexer is connected to R H C polarization and the second duplexer is connected to L H C polarization. Both the duplexers are connected to a receiver of channels varying 1 to 12 and 13 to 24 respectively. The duplexers are also connected from output multiplexer with channels varying from 1 to 12 and 13 to 24 respectively.