#

The input is as follows:

User selected coordinates.

Select location of P,

Cartesian, cylindrical. Cylindrical is selected.

R equals 3.125

Phi equals 155.16

Add vector V and select display options. Cartesian, cylindrical. Cartesian is selected.

V sub x equals negative 1.483

V sub y equals 2.793.

Display options

P, x equals negative 2.848. y equals 1.318. r equals 3.138. phi equals 155.16 degrees.

V, V sub x equals negative 1.483. V sub y equals 2.793. V sub r equals 2.519. V sub phi equals negative 1.912. display is selected.

The output is as follows:

An x y plane with different vectors. The x axis displays the values from negative 5 to 5 and the y axis displays the values from negative 5 to 5. The vectors V, V sub 0, V sub y, V, V sub r and V sub x start from common point (negative 2.8, 1.3). V sub x ends at (negative 4.5, 1.5). v sub y ends at (negative 2.8, 4.2). V sub rends at (negative 5. 1, 2.5), V ends at (negative 4.3, 4.5). All values are estimated.