#

The diagram shows a transmission line of length l, which connects to a generator on the left having a voltage source, V sub g through its sending-end ports. The voltage across these ports is V sub A A-prime. The receiving-end ports of the transmission line are connected to an R C circuit with a resistance R and capacitance C, with the voltage across the ports labeled V sub B B-prime. A rightward current, i, flows from port A to port B.