#

The circuit shows a transmission line with node A at load end and node C at the generator end. Node B is located in between, at a distance of l sub 1 equals 3 lambda over 8 from C and l sub 2 equals 5 lambda over 8 from A. The input impedance is Z sub in, with line impedance between C and B labeled Z sub 01 equals 100 ohms and between B and A labeled Z sub 02 equals 50 ohms. The load impedance is Z sub L equals (75 minus j 50) ohms.