#

The table data are as follows:

Fixed service:

Use, Commercial (C-band). Downlink frequency in MHz, 3,700 to 4,200. Uplink frequency in MHz, 5,925 to 6,425.

Use, Military (X-band). Downlink frequency in MHz, 7, 250 to 7,750. Uplink frequency in MHz, 7,900 to 8,400.

Use, Commercial (k-band) Domestic (USA). Downlink frequency in MHz, fixed service, 11,700 to 12,200. Uplink frequency in MHz, 14,000 to 14,500.

Use, Commercial (k-band) International. Downlink frequency in MHz, fixed service, 10,950 to 11,200. Uplink frequency in MHz, 27,500 to 31,000.

Mobile service:

Use, Maritime. Downlink frequency in MHz, 1,535 to 1,542 times 5. Uplink frequency in MHz, 1,635 to 1,644.

Use, Aeronautical. Downlink frequency in MHz, Mobile service, 1,542 times 5 to 1,558 times 8. Uplink frequency in MHz, 1,645 to 1,660.

Broadcast service:

Downlink frequency in MHz, 2,500 to 2,535 and 11,700 to 12,750. Uplink frequency in MHz, 2,655 to 2,690.

.

Telemetry, Tracking, and Command in MHz are 137 to 138, 401 to 402, and 1,525 to 1,540 respectively.