#

The drawing shows a feedline connected to a load with impedance Z sub L over nodes A, A-prime. The input impedance is Z sub in while feedline impedance is Z sub 01. A quarter-wave transformer of length, lambda over 4 is inserted between terminals M, M-prime and B, B-prime. The impedance of the transmission line between B, B-prime and A, A-prime is Z sub d, with d being the distance of B, B-prime from load.