#

The table shows the following data:

- Band, L F: R F ID frequency, 125 to 134 kilo hertz; Read range, less than or equal to 0.5 meters; Data rate, 1 kilobits per second; Typical applications- Animal ID, Automobile key and anti-theft, Access control

- Band, L F: R F ID frequency, 13.56 M hertz; Read range, less than or equal to 1.5 meters; Data rate, 25 kilobits per second; Typical applications- Smart cards, Article surveillance, Airline baggage tracking, Library book tracking

- Band, L F: R F ID frequency, 865 to 956 M hertz; Read range, less than or equal to 5 meters; Data rate, 30 kilobits per second; Typical applications – Supply chain management, Logistics

- Band, L F: R F ID frequency, 2.45 G hertz; Read range, less than or equal to 10 meters; Data rate, 100 kilobits per second; Typical applications- Vehicle toll collection, Railroad car monitoring