#

The wave pattern of E sub 1 (z, t) is with respect to negative z axis. The pattern has 4 cycles in which 2 cycles starts above the negative z axis and rest 2 cycles starts below the negative z axis. The cycle for omega t equals start fraction 3 pi over 2 end fraction starts from the origin and rises with a peak of 24 millivolts per meter at negative lambda over 4 and crosses the negative axis at negative lambda per 2, and a crest of negative 24 millivolts per meter at negative 3 lambda over 4. The cycle ends at negative lambda. The cycle for omega t equals start fraction pi over 2 end fraction starts from the origin and descends with a crest of negative 24 millivolts per meter at negative lambda over 4 and crosses the negative axis at negative lambda over 2, and a peak at negative 3 lambda over 4. The cycle ends at negative lambda. The cycle for omega t equals start fraction 5 pi over 4 end fraction starts from the origin and rises below the cycle of omega t equals start fraction 3 pi over 2 end fraction with a peak at negative lambda over 4 and crosses the negative axis at negative lambda over 2, and a crest at negative 3 lambda over 4. The cycle ends at negative lambda. The cycle for omega t equals start fraction pi over 4 end fraction starts from the origin and descends below the cycle of omega t equals start fraction pi over 2 end fraction with a crest at negative lambda over 4 and crosses the negative axis at negative lambda over 2, and a peak at negative 3 lambda over 4. The cycle ends at negative lambda.

The wave pattern of H sub (z, t) with respect to negative z axis shows 2 cycles. The cycle for omega t equals 0 starts above the origin at 64 micro amperes per meter, and a crest of negative 64 micro amperes per meter at negative lambda over 2, and a peak of 64 microamperes per meter at negative lambda. The cycle for omega t equals pi starts below the origin at negative 64 micro amperes per meter, and a peak of 64 micro amperes per meter at negative lambda over 2, and a crest of negative 64 microamperes per meter at negative lambda.