#

The screen on the left part of the module shows a wave moving in the z-direction, with its E component and H component shown at right angles to each other. The panel on the right shows the input and output parameters as follows:

Input:

Frequency, f equals 1.0 E9 Hertz

Relative permittivity, epsilon sub r equals 1.0

Relative permeability, micro sub r equals 1.0

Reference amplitude, E sub 0 equals 1.0 V per m

Reference phase, z equals 0, phi equals 0.0 rad

Length displayed, l equals 1.0 lambda

Output:

Wavelength, lambda equals 30.0 centimeters

Phase velocity, u sub p equals 3.0 times 10 to the 8th power meters per second

Period, T equals 1.0 times 10 raised to negative 9 seconds

Impedance of the medium in ohm

Eta equals 376.991118 plus j 0.0

Phase constants:

Beta equals 20.94395 per meter

Linear Polarization