#

The top left corner of the module shows two currents A and B of two dipole array.

The module displays a grapher at the top right corner that has two lobes along horizontal axis originates from 0 degrees to the 90 degrees.

The input of the two dipole array is shown at the bottom left corner of the module.

Maximum directivity 3.9606

Total radiated power 60.5975 [watts]

Plot: a radio button is on that reads E-H fields

A radio button is off that reads power

Instructions

Dipole lengths (wavelengths)

A 0.5 lambda

B 0.5 lambda

Phase difference

A radio button is on that reads deg

A radio button is off that reads rad

0.0

Distance between dipoles (wavelengths)

0.5 lambda

Max dipole current (amps)

A 1.0

B 1.0

The module displays a grapher at the bottom right corner that has two lobes along vertical axis originates from 90 degrees to the 0 degrees and 180 degrees.