#

The transmission line is shown as a rectangular circuit with two ports, A and A-prime labeled sending-end ports, and B and B-prime labeled receiving-end ports. The sending-end ports are connected to a generator circuit on the left consisting of an a c voltage source, V-tilde sub g, and an internal resistance Z sub g. The receiving-end ports are connected to a load circuit consisting of a load resistor Z sub L.