#

The table shows the following data:

- Parameter, R-prime: Coaxial, R sub s over 2 pi (1 over a plus 1 over b); two-wire, 2 R sub s over pi d; parallel-plate, 2 R sub s over w; unit, ohm per meter

- Parameter, L-prime: Coaxial, micro over 2 pi times natural logarithm of (b over a); two-wire, micro over pi times natural logarithm of [(upper D over d) plus the square root of (upper D over d) squared minus 1]; Parallel-plate, micro h over w; unit, H per meter

- Parameter, G-prime: Coaxial, 2 pi sigma over natural logarithm of (b over a); two-wire, pi times sigma over natural logarithm of [(upper D over d) plus the square root of (upper D over d) squared minus 1]; Parallel-plate, sigma w over h; unit, S per meter

- Parameter, C-prime: Coaxial, 2 pi epsilon over natural logarithm of (b over a); two-wire, start fraction pi times epsilon over natural logarithm of [(upper D over d) plus the square root of (upper D over d) squared minus 1] end fraction; Parallel-plate, epsilon w over h; unit, F per meter.