#

The illustration on the left shows a coaxial line with two cylindrical conductors placed one inside the other and connecting a generator to a load. The generator consists of a voltage source, V sub g, and a resistor R sub g, while the load consists of a resistor R sub L. The illustration on the right shows a cross-section of the coaxial line. Radial lines are drawn from the inner conductor to the other conductor, indicating the electric field lines, while concentric circles are drawn around the inner conductor, indicating the magnetic field lines.