#

The graph represents magnetic field H, in amperes per meter and electric field E, in volts per meter from 0.01 to 10000 on the left side of the vertical axis. While on the right side, the graph represents power density S, in watts per meter squared. The horizontal axis represents frequency in megahertz from 10 to the power of negative 2 to 10 to the fifth power. Three lines are drawn in the graph.

The line for electric field E starts from 614 volts per meter electric field and ends at 27.5 volts per meter electric field.

The line for magnetic field H starts from 163 amperes per meter magnetic field and ends at 0.0729 amperes per meter magnetic field.

The line for power density starts from 2 watts per meter squared power density and ends at 100 watts per meter squared power density.