#

- Material, Diamagnetic, Bismuth. Relative Permeability, mu sub r, 0.99983 approximate equals 1.

- Material, Diamagnetic, Gold. Relative Permeability, mu sub r, 0.99996 approximate equals 1.

- Material, Diamagnetic, Mercury. Relative Permeability, mu sub r, 0.99997 approximate equals 1.

- Material, Diamagnetic, Silver. Relative Permeability, mu sub r, 0.99998 approximate equals 1.

- Material, Diamagnetic, Copper. Relative Permeability, mu sub r, 0.99999 approximate equals 1.

- Material, Diamagnetic, Water. Relative Permeability, mu sub r, 0.99999 approximate equals 1.

- Material, Paramagnetic, Air. Relative Permeability, mu sub r, 1.000004 approximate equals 1.

- Material, Paramagnetic, Aluminum. Relative Permeability, mu sub r, 1.00002 approximate equals 1.

- Material, Paramagnetic, Tungsten. Relative Permeability, mu sub r, 1.00008 approximate equals 1.

- Material, Paramagnetic, Titanium. Relative Permeability, mu sub r, 1.0002 approximate equals 1.

- Material, Paramagnetic, Platinum. Relative Permeability, mu sub r, 1.0003 approximate equals 1.

- Material, Ferromagnetic (nonlinear), Cobalt. Relative Permeability, mu sub r, 250.

- Material, Ferromagnetic (nonlinear), Nickel. Relative Permeability, mu sub r, 600.

- Material, Ferromagnetic (nonlinear), Mild steel. Relative Permeability, mu sub r, 2,000.

- Material, Ferromagnetic (nonlinear), Iron (pure). Relative Permeability, mu sub r, 4,000 to 5,000.

- Material, Ferromagnetic (nonlinear), Silicon iron. Relative Permeability, mu sub r, 7,000.

- Material, Ferromagnetic (nonlinear), Mumetal. Relative Permeability, mu sub r, similar to 100,000.

- Material, Ferromagnetic (nonlinear), Purified iron. Relative Permeability, mu sub r, similar to 200,000.