#

The illustration shows a circuit where load terminal C is connected to load impedance, z sub L. Point B is marked on the transmission line at a distance of d sub min equals 0.125 lambda from point C.

The Smith chart shows the families of r sub L and x sub L circles. Point A is marked on the positive x-axis, with S value labeled 3.0. Point B is marked on the negative x-axis, representing voltage min. Point C is marked on a vertical line drawn downward from the origin, representing load and the distance between C and B is marked 0.125 lambda. An origin centered circle is drawn, passing through A, B, and C.