#

The left part of the screen shows an interactive Smith chart, with an S W R circle passing through two points. The right part of the screen shows the following checkboxes and output parameters:

Checkboxes ticked: S W R circle, Cursor lines, Show curves, Full Chart, Voltage maximum, Show gamma, Load

Parameters:

S W R equals 5.8284

D (max) equals 0.0625 lambda

D (min) equals 0.3125 lambda

z sub L equals 1.0 plus j 2.0

Gamma sub L equals 0.70710678, angle 45 degrees

z of d equals 0.604963 minus j 1.504591

Gamma sub d equals 0.70710678, angle negative 61.56 degrees

y of d equals 0.230043 plus j 0.572137

d equals 0.148 lambda

2 beta d minus 1.859823 rad minus 106.56 degrees

0.5 lambda minus d equals 0.352 lambda

2 beta (0.5 lambda minus d) equals 4.4234 rad equals 253.44 degrees

Set line: Z sub 0 equals 50.0 ohms

Set load: Z sub L equals 50.0 plus j 100.0 ohms