#

The drawing shows two parallel lines are placed horizontally between terminals and are further divided into small differential sections measuring delta z each in length. Each section shows a series connection of resistance R-prime delta z and inductance L-prime delta z on the top wire, and a parallel connection between top and bottom wires consisting of resistance G-prime delta z and capacitance C-prime delta z.